**

***PPUH DEXWAL***

*DOBROWODA 12,*

*28-100 BUSKO-ZDRÓJ*

[*www.dexwal.com*](http://www.dexwal.com/)

[*ppoz@dexwal.com*](mailto:ppoz@dexwal.com)

[*pp@dexwal.com*](mailto:pp@dexwal.com)

*+48 603 700 029*

*+48 601 964 069*

PRODUCT DATA SHEET:

Extinguishing lance

Product description:

The extinguishing lance is a device designed to extinguish fires in areas that are very difficult to reach, where it is not possible to administer an effective water jet with a normal nozzle. This is an indispensable tool for rescuers whose objective is to extinguish and prevent the spread of all kinds of fires where a water jet must be injected deep into the extinguished material (fires of barns, outbuildings, crops or peat bogs). Operating capacity is optimally 190 l/min; the water jet is cone-shaped. The stainless steel of which the extinguishing lance is made ensures that it is resistant not only to heat radiation but also to all kinds of mechanical damage, making it a durable and effective device even in the most difficult conditions. Thanks to its properties, it is resistant to erosion, oxidation and corrosion and the replaceable tip and tamper helps keep the tool in perfect condition at all times.

Lance elements / dimensions:

The lance itself weighs ?? kg and together with the extensions ?? kg, which is an additional advantage because it only takes one rescuer to move it.

Relatively small size (here I would write the length of the main module and the length of the extension)

It is designed for a working pressure of max 8bar

We can use the W 25 or W 52 hoses to supply the lance.

The product has been registered in the European Patent Office 2.